{"text_format":"3","workbook":"xls","n_sheets":7,"sheets":["封面","表1-1工程项目总价表 (2)"," 表1-2建筑工程分类分项工程量清单","表1-3设备采购和安装工程分类分项工程量清单","表1-4措施项目清单","表1-5其他项目清单","安全文明措施费分解表"],"not_rendered":{"external_links":1,"defined_names":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封面","index":0,"n_rows":17,"n_cols":3,"rows_kept":17,"merged":[[0,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[5,1,5,2],[5,3,5,6],[7,0,7,6],[8,0,8,6],[9,0,9,1],[9,2,9,5],[10,0,10,1],[11,2,12,5],[12,0,12,1],[13,0,13,1],[13,2,13,5],[14,0,14,1],[14,2,14,4],[14,5,14,6],[15,0,15,6],[16,2,16,5]],"flags":["formulas_cached_only"]}
[]
[]
["丰县大沙河水生态子午河水系贯通工程"]
[]
["工程量清单"]
{"$rows_empty":11}
["    编 制 时 间：",null,"2020-08-01"]

{"sheet":"表1-1工程项目总价表 (2)","index":1,"n_rows":87,"n_cols":6,"rows_kept":87,"merged":[[0,0,0,5],[1,0,1,3],[1,4,1,5],[2,2,2,4],[3,2,3,4],[4,2,4,4],[5,2,5,4],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,2,17,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[21,2,21,4],[22,2,22,4],[23,2,23,4],[24,2,24,4],[25,2,25,4],[26,2,26,4],[27,2,27,4],[28,2,28,4],[29,2,29,4],[30,2,30,4],[31,2,31,4],[32,2,32,4],[33,2,33,4],[34,2,34,4],[35,2,35,4],[36,2,36,4],[37,2,37,4],[38,2,38,4],[39,2,39,4],[40,2,40,4],[41,0,41,5],[43,3,43,5],[44,0,44,5],[45,0,45,3],[45,4,45,5],[46,2,46,4],[47,2,47,4],[48,2,48,4],[49,2,49,4],[50,2,50,4],[51,2,51,4],[52,2,52,4],[53,2,53,4],[54,2,54,4],[55,2,55,4],[56,2,56,4],[57,2,57,4],[58,2,58,4],[59,2,59,4],[60,2,60,4],[61,2,61,4],[62,2,62,4],[63,2,63,4],[64,2,64,4],[65,2,65,4],[66,2,66,4],[67,2,67,4],[68,2,68,4],[69,2,69,4],[70,2,70,4],[71,2,71,4],[72,2,72,4],[73,2,73,4],[74,2,74,4],[75,2,75,4],[76,2,76,4],[77,2,77,4],[78,2,78,4],[80,2,80,4],[81,2,81,4],[82,2,82,4],[83,2,83,4],[84,2,84,4],[85,2,85,4],[86,2,86,4]],"flags":["formulas_cached_only"]}
["工程项目总价表"]
["工程名称：丰县大沙河水生态子午河水系贯通工程",{"$nulls":3},"第1页 共2页"]
["序号","分类工程编码","工程项目名称",null,null,"金额（元）"]
["一",null,"建筑工程分类分项工程量清单项目"]
["1","50","水利工程"]
["1.1","5001","水利建筑工程"]
["1.1.1","500101","土方开挖工程"]
["1.1.2","500101","施工围堰工程"]
["1.2","5001","跌水1、3、4、5、6、7（共6座）"]
["1.2.1","500101","土方开挖工程"]
["1.2.2","500103","土石方填筑工程"]
["1.2.3","500109","混凝土工程"]
["1.2.4","500110","模板工程"]
["1.3","5001","跌水2"]
["1.3.1","500101","土方开挖工程"]
["1.3.2","500103","土石方填筑工程"]
["1.3.3","500109","混凝土工程"]
["1.3.4","500110","模板工程"]
["1.4","5001","跌水8、9、11、13、15、16、19、21、22（共9座）"]
["1.4.1","500101","土方开挖工程"]
["1.4.2","500103","土石方填筑工程"]
["1.4.3","500109","混凝土工程"]
["1.4.4","500110","模板工程"]
["1.5","5001","跌水10、12、14、16、18、20、23、24（共8座）"]
["1.5.1","500101","土方开挖工程"]
["1.5.2","500103","土石方填筑工程"]
["1.5.3","500109","混凝土工程"]
["1.5.4","500110","模板工程"]
["1.6","5001","陈庄东1桥"]
["1.6.1","500101","土方开挖工程"]
["1.6.2","500103","土石方填筑工程"]
["1.6.3","500108","基础防渗和地基加固工程"]
["1.6.4","500109","混凝土工程"]
["1.6.5","500111","钢筋加工及安装工程"]
["1.6.6","500110","模板工程"]
["1.6.7","500114","其他建筑工程"]
["1.7","5001","陈庄东2桥"]
["1.7.1","500101","土方开挖工程"]
["1.7.2","500103","土石方填筑工程"]
["1.7.3","500108","基础防渗和地基加固工程"]
["1.7.4","500109","混凝土工程"]
[]
[]
[]
["工程项目总价表"]
["工程名称：丰县大沙河水生态子午河水系贯通工程",{"$nulls":3},"第2页 共2页"]
["序号","分类工程编码","工程项目名称",null,null,"金额（元）"]
["1.7.5","500111","钢筋加工及安装工程"]
["1.7.6","500110","模板工程"]
["1.7.7","500114","其他建筑工程"]
["1.8","5001","杨五楼闸站"]
["1.8.1","500101","土方开挖工程"]
["1.8.2","500103","土石方填筑工程"]
["1.8.3","500109","混凝土工程"]
["1.8.4","500111","钢筋加工及安装工程"]
["1.8.5","500110","模板工程"]
["1.8.6","500114","其他建筑工程"]
["1.9","5001","杨五楼闸站对岸护坡"]
["1.9.1","500101","土方开挖工程"]
["1.9.2","500103","土石方填筑工程"]
["1.9.3","500109","混凝土工程"]
["1.9.4","500110","模板工程"]
["1.10","5001","杨五楼桥下护砌"]
["1.10.1","500101","土方开挖工程"]
["1.10.2","500103","土石方填筑工程"]
["1.10.3","500109","混凝土工程"]
["1.10.4","500110","模板工程"]
["1.11","5001","宋楼闸站维修"]
["1.11.1","500114","泵房维修"]
["1.11.2","500114","外墙围栏、护栏维修"]
["1.11.3","500114","闸上交通桥维修"]
["1.11.4","500114","围栏内绿化种植"]
["1.11.5","500114","宋楼闸站铜字制作安装"]
["二",null,"设备采购和安装工程分类分项工程量清单项目"]
["1","50","水利工程"]
["1.1","5002","水利安装工程"]
["1.1.1","500201","机电设备安装工程"]
["1.1.2","500202","金属结构设备安装工程"]
["三",null,"措施项目"]
[null,null,"安全文明措施",null,null,123692.78]
[null,null,"扬尘防控措施",null,null,24798.08]
["四",null,"预留金",null,null,"104739"]
["五",null,"零星工作项目",null,null,""]
[]
[]
[]
[null,null,"合计"]

{"sheet":" 表1-2建筑工程分类分项工程量清单","index":2,"n_rows":350,"n_cols":7,"rows_kept":350,"merged":[[0,0,0,6],[1,0,1,5],[2,3,2,4],[3,3,3,4],[4,3,4,4],[5,3,5,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4],[12,3,12,4],[13,3,13,4],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,3,18,4],[19,3,19,4],[20,3,20,4],[21,3,21,4],[22,3,22,4],[23,3,23,4],[24,3,24,4],[25,3,25,4],[26,3,26,4],[27,0,27,6],[28,0,28,5],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,3,37,4],[38,3,38,4],[39,3,39,4],[40,3,40,4],[41,3,41,4],[42,3,42,4],[43,3,43,4],[44,3,44,4],[45,3,45,4],[46,3,46,4],[47,3,47,4],[48,3,48,4],[49,3,49,4],[50,3,50,4],[51,3,51,4],[52,3,52,4],[53,3,53,4],[54,3,54,4],[55,3,55,4],[56,0,56,6],[57,0,57,5],[58,3,58,4],[59,3,59,4],[60,3,60,4],[61,3,61,4],[62,3,62,4],[63,3,63,4],[64,3,64,4],[65,3,65,4],[66,3,66,4],[67,3,67,4],[68,3,68,4],[69,3,69,4],[70,3,70,4],[71,3,71,4],[72,3,72,4],[73,3,73,4],[74,3,74,4],[75,3,75,4],[76,3,76,4],[77,3,77,4],[78,3,78,4],[79,3,79,4],[80,3,80,4],[81,3,81,4],[82,3,82,4],[83,3,83,4],[84,3,84,4],[85,3,85,4],[86,3,86,4],[87,0,87,6],[88,0,88,5],[89,3,89,4],[90,3,90,4],[91,3,91,4],[92,3,92,4],[93,3,93,4],[94,3,94,4],[95,3,95,4],[96,3,96,4],[97,3,97,4],[98,3,98,4],[99,3,99,4],[100,3,100,4],[101,3,101,4],[102,3,102,4],[103,3,103,4],[104,3,104,4],[105,3,105,4],[106,3,106,4],[107,3,107,4],[108,3,108,4],[109,3,109,4],[110,3,110,4],[111,3,111,4],[112,3,112,4],[113,3,113,4],[114,3,114,4],[115,0,115,6],[116,0,116,5],[117,3,117,4],[118,3,118,4],[119,3,119,4],[120,3,120,4],[121,3,121,4],[122,3,122,4],[123,3,123,4],[124,3,124,4],[125,3,125,4],[126,3,126,4],[127,3,127,4],[128,3,128,4],[129,3,129,4],[130,3,130,4],[131,3,131,4],[132,3,132,4],[133,3,133,4],[134,3,134,4],[135,3,135,4],[136,3,136,4],[137,3,137,4],[138,3,138,4],[139,3,139,4],[140,3,140,4],[141,0,141,6],[142,0,142,5],[143,3,143,4],[144,3,144,4],[145,3,145,4],[146,3,146,4],[147,3,147,4],[148,3,148,4],[149,3,149,4],[150,3,150,4],[151,3,151,4],[152,3,152,4],[153,3,153,4],[154,3,154,4],[155,3,155,4],[156,3,156,4],[157,3,157,4],[158,3,158,4],[159,3,159,4],[160,3,160,4],[161,3,161,4],[162,3,162,4],[163,3,163,4],[164,3,164,4],[165,3,165,4],[166,3,166,4],[167,3,167,4],[168,3,168,4],[169,3,169,4],[170,3,170,4],[171,3,171,4],[172,0,172,6],[173,0,173,5],[174,3,174,4],[175,3,175,4],[176,3,176,4],[177,3,177,4],[178,3,178,4],[179,3,179,4],[180,3,180,4],[181,3,181,4],[182,3,182,4],[183,3,183,4],[184,3,184,4],[185,3,185,4],[186,3,186,4],[187,3,187,4],[188,3,188,4],[189,3,189,4],[190,3,190,4],[191,3,191,4],[192,3,192,4],[193,3,193,4],[194,3,194,4],[195,3,195,4],[196,0,196,6],[197,0,197,5],[198,3,198,4],[199,3,199,4],[200,3,200,4],[201,3,201,4],[202,3,202,4],[203,3,203,4],[204,3,204,4],[205,3,205,4],[206,3,206,4],[207,3,207,4],[208,3,208,4],[209,3,209,4],[210,3,210,4],[211,3,211,4],[212,3,212,4],[213,3,213,4],[214,3,214,4],[215,3,215,4],[216,3,216,4],[217,3,217,4],[218,3,218,4],[219,3,219,4],[220,3,220,4],[221,3,221,4],[222,3,222,4],[223,3,223,4],[224,3,224,4],[225,0,225,6],[226,0,226,5],[227,3,227,4],[228,3,228,4],[229,3,229,4],[230,3,230,4],[231,3,231,4],[232,3,232,4],[233,3,233,4],[234,3,234,4],[235,3,235,4],[236,3,236,4],[237,3,237,4],[238,3,238,4],[239,3,239,4],[240,3,240,4],[241,3,241,4],[242,3,242,4],[243,3,243,4],[244,0,244,6],[245,0,245,6],[246,0,246,5],[247,3,247,4],[248,3,248,4],[249,3,249,4],[250,3,250,4],[251,3,251,4],[252,3,252,4],[253,3,253,4],[254,3,254,4],[255,3,255,4],[256,3,256,4],[257,3,257,4],[258,3,258,4],[259,3,259,4],[260,3,260,4],[261,3,261,4],[262,3,262,4],[263,3,263,4],[264,3,264,4],[265,3,265,4],[266,3,266,4],[267,3,267,4],[268,3,268,4],[269,3,269,4],[270,3,270,4],[271,3,271,4],[272,3,272,4],[273,0,273,6],[274,0,274,5],[275,3,275,4],[276,3,276,4],[277,3,277,4],[278,3,278,4],[279,3,279,4],[280,3,280,4],[281,3,281,4],[282,3,282,4],[283,3,283,4],[284,3,284,4],[285,3,285,4],[286,3,286,4],[287,3,287,4],[288,3,288,4],[289,3,289,4],[290,3,290,4],[291,3,291,4],[292,3,292,4],[293,3,293,4],[294,3,294,4],[295,3,295,4],[296,3,296,4],[297,3,297,4],[298,3,298,4],[299,3,299,4],[300,3,300,4],[301,3,301,4],[302,3,302,4],[303,0,303,6],[304,0,304,5],[305,3,305,4],[306,3,306,4],[307,3,307,4],[308,3,308,4],[309,3,309,4],[310,3,310,4],[311,3,311,4],[312,3,312,4],[313,3,313,4],[314,3,314,4],[315,3,315,4],[316,3,316,4],[317,3,317,4],[318,3,318,4],[319,3,319,4],[320,3,320,4],[321,3,321,4],[322,3,322,4],[323,3,323,4],[324,3,324,4],[325,3,325,4],[326,3,326,4],[327,3,327,4],[328,0,328,6],[329,0,329,5],[330,3,330,4],[331,3,331,4],[332,3,332,4],[333,3,333,4],[334,3,334,4],[335,3,335,4],[336,3,336,4],[337,3,337,4],[338,3,338,4],[339,3,339,4],[340,3,340,4],[341,3,341,4],[342,3,342,4],[343,3,343,4],[344,3,344,4],[345,3,345,4],[346,3,346,4],[347,3,347,4],[348,3,348,4],[349,3,349,4],[350,3,350,4],[351,3,351,4],[352,3,352,4],[353,3,353,4],[354,3,354,4],[355,3,355,4],[356,3,356,4],[357,3,357,4],[358,3,358,4],[359,3,359,4],[360,3,360,4],[361,0,361,6],[363,4,363,6]],"flags":["formulas_cached_only"]}
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1","50","水利工程",null,null,"1.000"]
["1.1","5001","水利建筑工程",null,null,"1.000"]
["1.1.1","500101","土方开挖工程",null,null,"1.000"]
["1.1.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.1.1.1.1","500101002001","原有子午河扩挖（K1+400-K3+720）\n1、土类分级：一二类土\n2、运距：河东堆土","m3",null,"52932.000"]
["1.1.1.1.2","500101002002","平地开河（K3+720-K5+900）河东堆土\n1、土类分级：一二类土\n2、运距：河东堆土","m3",null,"86319.000"]
["1.1.1.1.3","500101002003","平地开河（K3+720-K5+900）河西堆土\n1、土类分级：一二类土\n2、运距：0.6m3挖掘机挖装土自卸汽车运土 运距(km) ≤0.5 河东堆土","m3",null,"258535.000"]
["1.1.1.1.4","500101002004","大沙河西截渗沟清淤，子午河两侧各30m\n1、土类分级：一二类土\n2、运距：河东堆土","m3",null,"480.000"]
["1.1.1.1.5","500101002005","混播狗牙根、白三叶草籽（K1+400-K3+700）,护坡养护1年","m3",null,"95000.000"]
["1.1.2","500101","施工围堰工程",null,null,"1.000"]
["1.1.2.1","500101002","一般土方开挖",null,null,"1.000"]
["1.1.2.1.1","500101002014","填筑围堰","m3",null,"1500.000"]
["1.1.2.2","500103001","一般土方填筑",null,null,"1.000"]
["1.1.2.2.1","500103001009","拆除围堰","m3",null,"1500.000"]
["1.1.2.3","500114002","积水排除",null,null,"1.000"]
["1.1.2.3.1","500114002001","积水排除","m3",null,"203000.000"]
["1.2","5001","跌水1、3、4、5、6、7（共6座）",null,null,"1.000"]
["1.2.1","500101","土方开挖工程",null,null,"1.000"]
["1.2.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.2.1.1.1","500101002006","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"365.000"]
["1.2.2","500103","土石方填筑工程",null,null,"1.000"]
["1.2.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.2.2.1.1","500103001001","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"300.000"]
["1.2.2.2","500103007","垫层料填筑",null,null,"1.000"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.2.2.2.1","500103007001","砂垫层","m3",null,"27.900"]
["1.2.2.2.2","500103007002","碎石垫层","m3",null,"27.900"]
["1.2.3","500109","混凝土工程",null,null,"1.000"]
["1.2.3.1","500109001","普通混凝土",null,null,"1.000"]
["1.2.3.1.1","500109001001","C25砼护坡、护底\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"48.800"]
["1.2.3.1.2","500109001002","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"51.800"]
["1.2.3.1.3","500109001003","C25砼U型槽底板\n1、部位及类型：U型槽底板\n2、强度等级：C25","m3",null,"61.800"]
["1.2.3.1.4","500109001004","C25砼U型槽侧墙\n1、部位及类型：U型槽侧墙\n2、强度等级：C25","m3",null,"31.200"]
["1.2.3.1.5","500109001005","C25砼管涵基础\n1、部位及类型：管涵基础\n2、强度等级：C25","m3",null,"16.000"]
["1.2.3.1.6","500109001006","钢筋混凝土涵管铺设 管径(cm) 100","m",null,"36.000"]
["1.2.4","500110","模板工程",null,null,"1.000"]
["1.2.4.1","500110001","普通模板",null,null,"1.000"]
["1.2.4.1.1","500110001001","普通组合钢模板安装、拆除","m2",null,"665.300"]
["1.3","5001","跌水2",null,null,"1.000"]
["1.3.1","500101","土方开挖工程",null,null,"1.000"]
["1.3.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.3.1.1.1","500101002007","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"120.000"]
["1.3.2","500103","土石方填筑工程",null,null,"1.000"]
["1.3.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.3.2.1.1","500103001002","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"108.000"]
["1.3.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.3.2.2.1","500103007003","砂垫层","m3",null,"23.200"]
["1.3.2.2.2","500103007004","碎石垫层","m3",null,"23.200"]
["1.3.3","500109","混凝土工程",null,null,"1.000"]
["1.3.3.1","500109001","普通混凝土",null,null,"1.000"]
["1.3.3.1.1","500109001007","C25砼护坡、护底\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"41.400"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.3.3.1.2","500109001008","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"25.200"]
["1.3.4","500110","模板工程",null,null,"1.000"]
["1.3.4.1","500110001","普通模板",null,null,"1.000"]
["1.3.4.1.1","500110001002","普通组合钢模板安装、拆除","m2",null,"176.000"]
["1.4","5001","跌水8、9、11、13、15、16、19、21、22（共9座）",null,null,"1.000"]
["1.4.1","500101","土方开挖工程",null,null,"1.000"]
["1.4.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.4.1.1.1","500101002008","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"650.000"]
["1.4.2","500103","土石方填筑工程",null,null,"1.000"]
["1.4.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.4.2.1.1","500103001003","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"520.000"]
["1.4.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.4.2.2.1","500103007005","砂垫层","m3",null,"76.100"]
["1.4.2.2.2","500103007006","碎石垫层","m3",null,"23.200"]
["1.4.3","500109","混凝土工程",null,null,"1.000"]
["1.4.3.1","500109001","普通混凝土",null,null,"1.000"]
["1.4.3.1.1","500109001009","C25砼护坡、护底\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"183.600"]
["1.4.3.1.2","500109001010","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"204.100"]
["1.4.4","500110","模板工程",null,null,"1.000"]
["1.4.4.1","500110001","普通模板",null,null,"1.000"]
["1.4.4.1.1","500110001003","普通组合钢模板安装、拆除","m2",null,"1543.000"]
["1.5","5001","跌水10、12、14、16、18、20、23、24（共8座）",null,null,"1.000"]
["1.5.1","500101","土方开挖工程",null,null,"1.000"]
["1.5.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.5.1.1.1","500101002009","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"650.000"]
["1.5.2","500103","土石方填筑工程",null,null,"1.000"]
["1.5.2.1","500103001","一般土方填筑",null,null,"1.000"]
[]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.5.2.1.1","500103001004","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm","m3",null,"520.000"]
["1.5.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.5.2.2.1","500103007007","砂垫层","m3",null,"41.500"]
["1.5.2.2.2","500103007008","碎石垫层","m3",null,"41.500"]
["1.5.3","500109","混凝土工程",null,null,"1.000"]
["1.5.3.1","500109001","普通混凝土",null,null,"1.000"]
["1.5.3.1.1","500109001011","C25砼护坡、护底\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"71.600"]
["1.5.3.1.2","500109001012","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"69.100"]
["1.5.3.1.3","500109001013","C25砼U型槽底板\n1、部位及类型：U型槽底板\n2、强度等级：C25","m3",null,"104.500"]
["1.5.3.1.4","500109001014","C25砼U型槽侧墙\n1、部位及类型：U型槽侧墙\n2、强度等级：C25","m3",null,"52.900"]
["1.5.3.1.5","500109001015","C25砼管涵基础\n1、部位及类型：管涵基础\n2、强度等级：C25","m3",null,"8.100"]
["1.5.3.1.6","500109001016","混凝土及钢筋混凝土涵管铺设 管径(cm) 60","m",null,"48.000"]
["1.5.3.1.7","500109001017","砼栏杆","m",null,"48.000"]
["1.5.4","500110","模板工程",null,null,"1.000"]
["1.5.4.1","500110001","普通模板",null,null,"1.000"]
["1.5.4.1.1","500110001004","普通组合钢模板安装、拆除 底部结构","m2",null,"504.000"]
["1.5.4.1.2","500110001005","普通组合钢模板安装、拆除 中、上部结构","m2",null,"446.000"]
["1.6","5001","陈庄东1桥",null,null,"1.000"]
["1.6.1","500101","土方开挖工程",null,null,"1.000"]
["1.6.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.6.1.1.1","500101002010","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"50.100"]
["1.6.2","500103","土石方填筑工程",null,null,"1.000"]
["1.6.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.6.2.1.1","500103001005","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"40.000"]
["1.6.2.2","500103007","垫层料填筑",null,null,"1.000"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.6.2.2.1","500103007009","砂垫层","m3",null,"0.600"]
["1.6.2.2.2","500103007010","碎石垫层","m3",null,"0.600"]
["1.6.3","500108","基础防渗和地基加固工程",null,null,"1.000"]
["1.6.3.1","500108004","混凝土灌注桩",null,null,"1.000"]
["1.6.3.1.1","500108004001","灌注桩工作平台打拆","m2",null,"400.000"]
["1.6.3.1.2","500108004002","护筒制作 桩径100cm","根",null,"10.000"]
["1.6.3.1.3","500108004003","灌注桩钻孔","100m进深",null,"2.480"]
["1.6.3.1.4","500108004009","钢筋制作安装 灌注桩钢筋笼(片)制安","t",null,"22.400"]
["1.6.3.1.5","500108004004","灌注桩混凝土","m3",null,"195.000"]
["1.6.4","500109","混凝土工程",null,null,"1.000"]
["1.6.4.1","500109001","普通混凝土",null,null,"1.000"]
["1.6.4.1.1","500109001018","C25砼护坡\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"0.900"]
["1.6.4.1.2","500109001019","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"2.500"]
["1.6.4.1.3","500109001020","C30砼帽梁、墩柱\n1、部位及类型：帽梁、墩柱\n2、强度等级：C30","m3",null,"53.000"]
["1.6.4.1.4","500109001021","C50砼桥面预制板制作与安装\n1、部位及类型：桥面\n2、强度等级：C50\n3、模板脚手架摊销","m3",null,"129.000"]
["1.6.4.1.5","500109001022","C50砼桥面铺装层\n1、部位及类型：桥面铺装层\n2、强度等级：C50","m3",null,"39.000"]
["1.6.4.1.6","500109001023","C30砼防撞护栏、护车带\n1、部位及类型：防撞护栏、护车带\n2、强度等级：C30","m3",null,"37.100"]
["1.6.4.1.7","500109001024","C30砼耳墙\n1、部位及类型：耳墙\n2、强度等级：C30","m3",null,"8.000"]
["1.6.4.1.8","500109001025","C30砼搭板\n1、部位及类型：搭板\n2、强度等级：C30","m3",null,"21.000"]
["1.6.4.1.9","500109001026","C30砼垫石\n1、部位及类型：砼垫石\n2、强度等级：C30","m3",null,"0.700"]
["1.6.5","500111","钢筋加工及安装工程",null,null,"1.000"]
["1.6.5.1","500111001","钢筋制作安装",null,null,"1.000"]
[]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.6.5.1.1","500111001001","钢筋制作安装\n各种牌号、型号及规格的钢筋加工及安装，包含运输","t",null,"38.000"]
["1.6.5.1.2","500111001002","预应力钢筋制作、安装\n各种牌号、型号及规格的钢筋加工及安装，包含运输","t",null,"2.500"]
["1.6.6","500110","模板工程",null,null,"1.000"]
["1.6.6.1","500110001","普通模板",null,null,"1.000"]
["1.6.6.1.1","500110001007","普通组合钢模板安装、拆除 中、上部结构","m2",null,"433.000"]
["1.6.7","500114","其他建筑工程",null,null,"1.000"]
["1.6.7.1","500114001","其他永久建筑工程",null,null,"1.000"]
["1.6.7.1.1","500114001001","橡胶支座\n1、板式橡胶支（150mm×250mm×35mm）","块",null,"80.000"]
["1.6.7.1.2","500114001002","铭牌制作与安装","项",null,"1.000"]
["1.6.7.1.3","500114001003","限载标志","座",null,"2.000"]
["1.6.7.1.4","500114001004","伸缩缝\n1、GQF-F-6型伸缩装置","m",null,"30.000"]
["1.6.7.1.5","500114001005","Φ10PVC泄水管（间距400cm）、沉降缝等其他零星工程","项",null,"1.000"]
["1.6.7.1.6","500114001006","5cm厚沥青砼磨耗层","m2",null,"312.000"]
["1.6.7.1.7","500114001007","水泥稳定碎石 厂拌机铺 厚度20cm","m2",null,"55.000"]
["1.6.7.1.8","500114001008","30cm厚12%石灰稳定土","m2",null,"55.000"]
["1.7","5001","陈庄东2桥",null,null,"1.000"]
["1.7.1","500101","土方开挖工程",null,null,"1.000"]
["1.7.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.7.1.1.1","500101002011","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"74.000"]
["1.7.2","500103","土石方填筑工程",null,null,"1.000"]
["1.7.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.7.2.1.1","500103001006","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"59.000"]
["1.7.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.7.2.2.1","500103007011","砂垫层","m3",null,"0.600"]
["1.7.2.2.2","500103007012","碎石垫层","m3",null,"0.600"]
["1.7.3","500108","基础防渗和地基加固工程",null,null,"1.000"]
["1.7.3.1","500108004","混凝土灌注桩",null,null,"1.000"]
["1.7.3.1.1","500108004005","灌注桩工作平台打拆","m2",null,"450.000"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.7.3.1.2","500108004006","护筒制作 桩径100cm","根",null,"10.000"]
["1.7.3.1.3","500108004007","灌注桩钻孔","100m进深",null,"2.720"]
["1.7.3.1.4","500108004010","钢筋制作安装 灌注桩钢筋笼(片)制安","t",null,"25.600"]
["1.7.3.1.5","500108004008","灌注桩混凝土","m3",null,"213.200"]
["1.7.4","500109","混凝土工程",null,null,"1.000"]
["1.7.4.1","500109001","普通混凝土",null,null,"1.000"]
["1.7.4.1.1","500109001027","C25砼护坡\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"0.900"]
["1.7.4.1.2","500109001028","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"2.500"]
["1.7.4.1.3","500109001029","C30砼帽梁、墩柱\n1、部位及类型：帽梁、墩柱\n2、强度等级：C30","m3",null,"64.200"]
["1.7.4.1.4","500109001030","C50砼桥面预制板制作与安装\n1、部位及类型：桥面\n2、强度等级：C50\n3、模板脚手架摊销","m3",null,"152.900"]
["1.7.4.1.5","500109001031","C50砼桥面铺装层\n1、部位及类型：桥面铺装层\n2、强度等级：C50","m3",null,"47.300"]
["1.7.4.1.6","500109001032","C30砼防撞护栏、护车带\n1、部位及类型：防撞护栏、护车带\n2、强度等级：C30","m3",null,"38.100"]
["1.7.4.1.7","500109001033","C30砼耳墙\n1、部位及类型：耳墙\n2、强度等级：C30","m3",null,"10.600"]
["1.7.4.1.8","500109001034","C30砼搭板\n1、部位及类型：搭板\n2、强度等级：C30","m3",null,"24.400"]
["1.7.4.1.9","500109001035","C30砼垫石\n1、部位及类型：砼垫石\n2、强度等级：C30","m3",null,"1.000"]
["1.7.5","500111","钢筋加工及安装工程",null,null,"1.000"]
["1.7.5.1","500111001","钢筋制作安装",null,null,"1.000"]
["1.7.5.1.1","500111001003","钢筋制作安装\n各种牌号、型号及规格的钢筋加工及安装，包含运输","t",null,"45.200"]
["1.7.5.1.2","500111001004","预应力钢筋制作、安装\n各种牌号、型号及规格的钢筋加工及安装，包含运输","t",null,"3.000"]
["1.7.6","500110","模板工程",null,null,"1.000"]
["1.7.6.1","500110001","普通模板",null,null,"1.000"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.7.6.1.1","500110001008","普通组合钢模板安装、拆除 中、上部结构","m2",null,"423.000"]
["1.7.7","500114","其他建筑工程",null,null,"1.000"]
["1.7.7.1","500114001","其他永久建筑工程",null,null,"1.000"]
["1.7.7.1.1","500114001009","橡胶支座\n1、板式橡胶支（150mm×250mm×35mm）","块",null,"80.000"]
["1.7.7.1.2","500114001010","铭牌制作与安装","项",null,"1.000"]
["1.7.7.1.3","500114001011","限载标志","座",null,"2.000"]
["1.7.7.1.4","500114001012","伸缩缝\n1、GQF-F-6型伸缩装置","m",null,"37.250"]
["1.7.7.1.5","500114001013","Φ10PVC泄水管（间距400cm）、沉降缝等其他零星工程","项",null,"1.000"]
["1.7.7.1.6","500114001014","5cm厚沥青砼磨耗层","m2",null,"364.000"]
["1.7.7.1.7","500114001015","水泥稳定碎石 厂拌机铺 厚度20cm","m2",null,"70.000"]
["1.7.7.1.8","500114001016","30cm厚12%石灰稳定土","m2",null,"70.000"]
["1.8","5001","杨五楼闸站",null,null,"1.000"]
["1.8.1","500101","土方开挖工程",null,null,"1.000"]
["1.8.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.8.1.1.1","500101002012","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"790.000"]
["1.8.2","500103","土石方填筑工程",null,null,"1.000"]
["1.8.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.8.2.1.1","500103001007","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"610.000"]
["1.8.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.8.2.2.1","500103007013","砂垫层","m3",null,"22.200"]
["1.8.2.2.2","500103007014","碎石垫层","m3",null,"22.200"]
["1.8.3","500109","混凝土工程",null,null,"1.000"]
["1.8.3.1","500109001","普通混凝土",null,null,"1.000"]
["1.8.3.1.1","500109001036","C25砼垫层封底\n1、部位及类型：垫层封底\n2、强度等级：C25","m3",null,"16.100"]
["1.8.3.1.2","500109001037","C25砼护底、护坡、支墩\n1、部位及类型：护底、护坡、支墩\n2、强度等级：C25","m3",null,"42.500"]
["1.8.3.1.3","500109001038","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"27.100"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.8.3.1.4","500109001039","C25砼泵房基础\n1、部位及类型：泵房基础\n2、强度等级：C25","m3",null,"29.500"]
["1.8.3.1.5","500109001040","C25砼进水池底板\n1、部位及类型：进水池底板\n2、强度等级：C25","m3",null,"7.700"]
["1.8.3.1.6","500109001041","C25砼进水池侧墙\n1、部位及类型：进水池侧墙\n2、强度等级：C25","m3",null,"27.400"]
["1.8.3.1.7","500109001042","C25砼出水池底板\n1、部位及类型：出水池底板\n2、强度等级：C25","m3",null,"5.600"]
["1.8.3.1.8","500109001043","C25砼出水池侧墙\n1、部位及类型：出水池侧墙\n2、强度等级：C25","m3",null,"10.500"]
["1.8.3.1.9","500109001044","C25砼检查井底板\n1、部位及类型：检查井底板\n2、强度等级：C25","m3",null,"2.700"]
["1.8.3.1.10","500109001045","C25砼检查井侧墙\n1、部位及类型：检查井侧墙\n2、强度等级：C25","m3",null,"5.600"]
["1.8.3.1.11","500109001046","C25砼U型槽底板\n1、部位及类型：U型槽底板\n2、强度等级：C25","m3",null,"6.700"]
["1.8.3.1.12","500109001047","C25砼U型槽侧墙\n1、部位及类型：U型槽侧墙\n2、强度等级：C25","m3",null,"4.400"]
["1.8.3.1.13","500109001057","C25砼闸室底板\n1、部位及类型：闸室底板\n2、强度等级：C25","m3",null,"13.700"]
["1.8.3.1.14","500109001058","C25砼闸室侧墙\n1、部位及类型：闸室侧墙\n2、强度等级：C25","m3",null,"24.700"]
["1.8.3.1.15","500109001048","C25砼上游连接段底板\n1、部位及类型：上游连接段底板\n2、强度等级：C25","m3",null,"8.800"]
["1.8.3.1.16","500109001049","C25砼上游连接段侧墙\n1、部位及类型：上游连接段侧墙\n2、强度等级：C25","m3",null,"12.000"]
["1.8.3.1.17","500109001050","C25砼下游连接段底板\n1、部位及类型：下游连接段底板\n2、强度等级：C25","m3",null,"21.700"]
[]
[]
[]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.8.3.1.18","500109001051","C25砼下游连接段侧墙\n1、部位及类型：下游连接段底板\n2、强度等级：C25","m3",null,"22.800"]
["1.8.3.1.19","500109001052","C25砼挡墙底板\n1、部位及类型：挡墙底板\n2、强度等级：C25","m3",null,"5.900"]
["1.8.3.1.20","500109001053","C25砼挡墙侧墙\n1、部位及类型：挡墙侧墙\n2、强度等级：C25","m3",null,"6.500"]
["1.8.3.1.21","500109001054","C25砼排架、启闭机梁\n1、部位及类型：排架、启闭机梁\n2、强度等级：C25","m3",null,"4.500"]
["1.8.3.1.22","500109001055","C25砼管涵基础\n1、部位及类型：管涵基础\n2、强度等级：C25","m3",null,"5.500"]
["1.8.3.1.23","500109001056","钢筋混凝土涵管铺设 管径(cm) 100","m",null,"10.000"]
["1.8.4","500111","钢筋加工及安装工程",null,null,"1.000"]
["1.8.4.1","500111001","钢筋制作安装",null,null,"1.000"]
["1.8.4.1.1","500111001005","钢筋制作安装\n各种牌号、型号及规格的钢筋加工及安装，包含运输","t",null,"13.920"]
["1.8.5","500110","模板工程",null,null,"1.000"]
["1.8.5.1","500110001","普通模板",null,null,"1.000"]
["1.8.5.1.1","500110001009","普通组合钢模板安装、拆除 底部结构","m2",null,"87.000"]
["1.8.5.1.2","500110001010","普通组合钢模板安装、拆除 中、上部结构","m2",null,"647.000"]
["1.8.6","500114","其他建筑工程",null,null,"1.000"]
["1.8.6.1","500114001","其他永久建筑工程",null,null,"1.000"]
["1.8.6.1.1","500114001017","框架结构泵房\n1、详见图纸","m2",null,"34.000"]
["1.8.6.1.2","500114001018","钢管栏杆\n1、钢管φ50×2.5","m",null,"15.000"]
["1.8.6.1.3","500114001019","砼栏杆\n1、部位及类型：栏杆\n2、强度等级：C25","m",null,"40.000"]
["1.8.6.1.4","500114001020","钢爬梯\n1、型号：T1 06","座",null,"1.000"]
["1.8.6.1.5","500114001021","止水 塑料止水带(100m)\n1、型号：651型300-（8-15）","m",null,"18.000"]
["1.8.6.1.6","500114001022","沉降缝","项",null,"1.000"]
["1.8.6.1.7","500114001023","原有闸站拆除","项",null,"1.000"]
["1.9","5001","杨五楼闸站对岸护坡",null,null,"1.000"]
["1.9.1","500101","土方开挖工程",null,null,"1.000"]
["1.9.1.1","500101002","一般土方开挖",null,null,"1.000"]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.9.1.1.1","500101002015","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"150.000"]
["1.9.2","500103","土石方填筑工程",null,null,"1.000"]
["1.9.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.9.2.1.1","500103001010","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"120.000"]
["1.9.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.9.2.2.1","500103007017","砂垫层","m3",null,"25.000"]
["1.9.2.2.2","500103007018","碎石垫层","m3",null,"25.000"]
["1.9.3","500109","混凝土工程",null,null,"1.000"]
["1.9.3.1","500109001","普通混凝土",null,null,"1.000"]
["1.9.3.1.1","500109001066","C25砼护坡、护底\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"42.900"]
["1.9.3.1.2","500109001067","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"35.300"]
["1.9.4","500110","模板工程",null,null,"1.000"]
["1.9.4.1","500110001","普通模板",null,null,"1.000"]
["1.9.4.1.1","500110001012","普通组合钢模板安装、拆除","m2",null,"294.000"]
["1.10","5001","杨五楼桥下护砌",null,null,"1.000"]
["1.10.1","500101","土方开挖工程",null,null,"1.000"]
["1.10.1.1","500101002","一般土方开挖",null,null,"1.000"]
["1.10.1.1.1","500101002013","土方开挖\n1、土类分级：一二类土\n2、运距：堆土区自行考虑","m3",null,"28.000"]
["1.10.2","500103","土石方填筑工程",null,null,"1.000"]
["1.10.2.1","500103001","一般土方填筑",null,null,"1.000"]
["1.10.2.1.1","500103001008","土方回填、压实\n1、土质及含水量:一二类土\n2、分层厚度及碾压遍数:分层压实20~30cm\n3、压实度:详见图纸","m3",null,"25.000"]
["1.10.2.2","500103007","垫层料填筑",null,null,"1.000"]
["1.10.2.2.1","500103007015","砂垫层","m3",null,"5.100"]
["1.10.2.2.2","500103007016","碎石垫层","m3",null,"5.100"]
["1.10.3","500109","混凝土工程",null,null,"1.000"]
["1.10.3.1","500109001","普通混凝土",null,null,"1.000"]
[]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.10.3.1.1","500109001059","C25砼护坡、护底\n1、部位及类型：护底、护坡\n2、强度等级：C25","m3",null,"8.400"]
["1.10.3.1.2","500109001060","C25砼格埂\n1、部位及类型：格埂\n2、强度等级：C25","m3",null,"8.800"]
["1.10.4","500110","模板工程",null,null,"1.000"]
["1.10.4.1","500110001","普通模板",null,null,"1.000"]
["1.10.4.1.1","500110001011","普通组合钢模板安装、拆除","m2",null,"59.100"]
["1.11","5001","宋楼闸站维修",null,null,"1.000"]
["1.11.1","500114","泵房维修",null,null,"1.000"]
["1.11.1.1","500114001","外墙刷漆",null,null,"1.000"]
["1.11.1.1.1","500114001024","大墙溶剂涂料毛面 1底2面","m2",null,"661.500"]
["1.11.1.1.2","500114001025","女儿墙溶剂涂料毛面 1底2面","m2",null,"97.200"]
["1.11.1.2","500114001","其他工程",null,null,"1.000"]
["1.11.1.2.1","500114001026","更换外门（2扇）","m2",null,"5.200"]
["1.11.1.2.2","500114001027","更换窗玻璃（3个）","m2",null,"15.700"]
["1.11.1.2.3","500114001028","屋面防水\n1、卷材屋面 SBS改性沥青防水卷材 冷粘法 双层\n2、刚性防水屋面 细石混凝土 有分格缝 40mm厚","m2",null,"238.000"]
["1.11.1.3","500109001","电缆沟盖板制作安装",null,null,"1.000"]
["1.11.1.3.1","500109001061","C25钢筋砼（880×580×60㎜）\n1、部位及类型：预制砼盖板\n2、强度等级：C25","m3",null,"0.200"]
["1.11.1.3.2","500109001062","C25钢筋砼（860×380×60㎜）\n1、部位及类型：预制砼盖板\n2、强度等级：C25","m3",null,"0.100"]
["1.11.1.3.3","500111001006","钢筋制作安装","t",null,"0.007"]
["1.11.1.4","500109001","检修闸门槽口盖板制作安装",null,null,"1.000"]
["1.11.1.4.1","500109001063","C25钢筋砼（750×500×60㎜）\n1、部位及类型：预制砼盖板\n2、强度等级：C25","m3",null,"0.100"]
["1.11.1.4.2","500111001007","钢筋制作安装","t",null,"0.021"]
[]
["建筑工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量单位",null,"工程数量","备注"]
["1.11.1.4.3","500114001029","二楼沉降缝维修","项",null,"1.000"]
["1.11.2","500114","外墙围栏、护栏维修",null,null,"1.000"]
["1.11.2.1","500114001","外墙围栏、护栏维修",null,null,"1.000"]
["1.11.2.1.1","500114001030","围栏更换\n1、1.5米高罗马柱围栏购置安装","m",null,"10.000"]
["1.11.2.1.2","500114001031","护栏刷漆\n1、护栏尺寸1.5×0.9m","m2",null,"297.000"]
["1.11.3","500114","闸上交通桥维修",null,null,"1.000"]
["1.11.3.1","500109001","闸上交通桥维修",null,null,"1.000"]
["1.11.3.1.1","500109001064","C30砼桥面铺装\n1、部位及类型：桥面铺装\n2、强度等级：C30","m3",null,"33.800"]
["1.11.3.1.2","500109001065","C25砼翼墙维修\n1、翼墙按原标准维修损坏部分","m3",null,"10.000"]
["1.11.3.1.3","500111001008","钢筋制作安装","t",null,"2.630"]
["1.11.3.1.4","500114001032","防撞护栏不锈钢牛角护栏","项",null,"1.000"]
["1.11.3.1.5","500114001036","排水管","项",null,"1.000"]
["1.11.4","500114","围栏内绿化种植",null,null,"1.000"]
["1.11.4.1","500114001","围栏内绿化种植",null,null,"1.000"]
["1.11.4.1.1","500114001033","护坡草皮铺种 铺草皮 满铺（含养护）","m2",null,"1500.000"]
["1.11.4.1.2","500114001034","绿化树购买栽植（银杏、女贞、金桂、樱花）","棵",null,"50.000"]
["1.11.5","500114","宋楼闸站铜字制作安装",null,null,"1.000"]
["1.11.5.1","500114001","宋楼闸站铜字制作安装",null,null,"1.000"]
["1.11.5.1.1","500114001035","宋楼闸站铜字制作安装","m2",null,"1.000"]

{"sheet":"表1-3设备采购和安装工程分类分项工程量清单","index":3,"n_rows":34,"n_cols":7,"rows_kept":34,"merged":[[0,0,0,6],[1,0,1,5],[2,4,2,5],[3,4,3,5],[4,4,4,5],[5,4,5,5],[6,4,6,5],[7,4,7,5],[8,4,8,5],[9,4,9,5],[10,4,10,5],[11,4,11,5],[12,4,12,5],[13,4,13,5],[14,4,14,5],[15,4,15,5],[16,4,16,5],[17,4,17,5],[18,4,18,5],[19,4,19,5],[20,4,20,5],[21,4,21,5],[22,0,23,0],[22,1,23,1],[22,2,23,2],[22,3,23,3],[22,4,23,5],[22,6,23,6],[24,4,24,5],[25,0,25,6],[26,5,26,6],[27,0,27,6],[28,0,28,5],[29,4,29,5],[30,4,30,5],[31,4,31,5],[32,4,32,5],[33,4,33,5],[34,4,34,5],[35,4,35,5],[36,4,36,5],[37,4,37,5],[38,4,38,5],[39,4,39,5],[40,4,40,5],[41,4,41,5],[42,4,42,5],[43,4,43,5],[44,4,44,5],[45,4,45,5],[46,4,46,5],[47,4,47,5],[48,4,48,5],[49,4,49,5],[50,4,50,5],[51,4,51,5],[52,4,52,5],[53,4,53,5],[54,4,54,5],[55,4,55,5],[56,4,56,5],[57,4,57,5],[58,4,58,5],[59,4,59,5],[60,4,60,5],[61,4,61,5],[62,4,62,5],[63,4,63,5],[64,4,64,5],[65,4,65,5],[66,4,66,5],[67,0,67,6],[69,5,69,6]],"flags":["formulas_cached_only"]}
["设备采购和安装工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量\n单位","工程\n数量",null,"备注"]
["1","50","水利工程",null,"1.000"]
["1.1","5002","水利安装工程",null,"1.000"]
["1.1.1","500201","机电设备安装工程",null,"1.000"]
["1.1.1.1","500201002","杨五楼闸站",null,"1.000"]
["1.1.1.1.1","500201002001","350HWG-8混流泵购置安装\n1、含泵体、泵座、拍门等辅件","台","2.000"]
["1.1.1.1.2","500201005001","30KW电机购置安装\n1、30KW（Y220L-4）电机购置安装\n2、含与水泵配合的辅件，含水泵与电机连接电缆30m","台","2.000"]
["1.1.1.1.3","500201013002","真空泵购置、安装\n1、SZG-8型真空泵安装\n2、含连接管道、阀门等辅件","台","1.000"]
["1.1.1.1.4","500201013003","DN350电磁流量计\n1、电磁流量计DN350购置安装，含连接管件、附件等图示全部内容","个","2.000"]
["1.1.1.1.5","500201013004","DN350伸缩节","个","2.000"]
["1.1.1.1.6","500201021001","100KVA变压器购置安装（含变压器基础）\n1、S13-M-100/10变压器(100KVA)购置安装，含铜芯","台","1.000",null,"详见图纸"]
["1.1.1.1.7","500201021002","变压器入户手续及其他费用","项","1.000"]
["1.1.1.1.8","500201024001","配电柜购置（1台30KW）\n1、配套单台30KW泵站全套电气柜\n2、含配电柜底座及其它附件","台","2.000",null,"详见图纸"]
["1.1.1.1.9","500201018001","配电柜至变压器电缆购置安装 30m","m","30.000",null,"详见图纸"]
["1.1.1.1.10","500201018002","变压器以上电缆10kv购置安装 50m","m","50.000",null,"详见图纸"]
["1.1.1.1.11","500201020001","接地装置制作安装 制作及安装","t","0.050"]
["1.1.2","500202","金属结构设备安装工程",null,"1.000"]
["1.1.2.1","500202005","杨五楼闸站",null,"1.000"]
["1.1.2.1.1","500202005001","铸铁镶铜闸门（2x2.5m）","扇","1.000"]
["1.1.2.1.2","500202003001","手电两用螺杆式启闭机购置安装8t\n1、含螺杆、支架及其他辅件","台","1.000"]
["1.1.2.1.3","500202008001","DN350泵管（铸铁、含防腐、法兰、弯头等）\n1、铸铁管DN350，壁厚不小于10mm，2、含法兰（厚度不小于21mm）、胶圈、螺栓等辅件","m","36.000"]
[]
["1.1.2.2","500202005","宋楼闸站维修",null,"1.000"]
[]
[]
["设备采购和安装工程分类分项工程量清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程"]
["序号","项目编码","项目名称","计量\n单位","工程\n数量",null,"备注"]
["1.1.2.2.1","500202003002","启闭机的启动柜（型号：GEX 规格：600×500）","台","3.000"]
["1.1.2.2.2","500202003003","1米宽橡胶绝缘垫","m","50.000"]
["1.1.2.2.3","500202003004","绝缘手套、绝缘靴","套","2.000"]
["1.1.2.2.4","500202003005","照明灯管","套","30.000"]

{"sheet":"表1-4措施项目清单","index":4,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,4],[1,0,1,3],[2,1,2,2],[2,3,2,4],[3,1,3,2],[3,3,3,4],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,1,35,2],[35,3,35,4],[36,1,36,2],[36,3,36,4],[37,1,37,2],[37,3,37,4],[38,1,38,2],[38,3,38,4],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,0,41,4],[43,2,43,4]],"flags":["formulas_cached_only"]}
["措施项目清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程",{"$nulls":3},"第1页 共1页"]
["序号","项目名称",null,"备注"]
["1","安全文明措施",null,123692.78]
["2","扬尘防控措施",null,24798.08]
["3","临时工程"]
["4","保险费"]

{"sheet":"表1-5其他项目清单","index":5,"n_rows":4,"n_cols":5,"rows_kept":4,"merged":[[0,0,0,4],[1,0,1,3],[2,1,2,2],[2,3,2,4],[3,1,3,2],[3,3,3,4],[4,1,4,2],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,16,2],[16,3,16,4],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,1,35,2],[35,3,35,4],[36,1,36,2],[36,3,36,4],[37,1,37,2],[37,3,37,4],[38,1,38,2],[38,3,38,4],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,0,41,4],[43,2,43,4]],"flags":["formulas_cached_only"]}
["其他项目清单"]
["工程名称：丰县大沙河水生态子午河水系贯通工程",{"$nulls":3},"第1页 共1页"]
["序号","项目名称",null,"备注"]
["1","预留金",null,104738.82]

{"sheet":"安全文明措施费分解表","index":6,"n_rows":37,"n_cols":9,"rows_kept":37,"merged":[[0,0,0,8],[1,0,1,7],[2,5,2,6],[2,7,2,8],[3,5,3,6],[3,7,3,8],[4,5,4,6],[4,7,4,8],[5,5,5,6],[5,7,5,8],[6,5,6,6],[6,7,6,8],[7,5,7,6],[7,7,7,8],[8,5,8,6],[8,7,8,8],[9,5,9,6],[9,7,9,8],[10,5,10,6],[10,7,10,8],[11,5,11,6],[11,7,11,8],[12,5,12,6],[12,7,12,8],[13,5,13,6],[13,7,13,8],[14,5,14,6],[14,7,14,8],[15,5,15,6],[15,7,15,8],[16,5,16,6],[16,7,16,8],[17,5,17,6],[17,7,17,8],[18,5,18,6],[18,7,18,8],[19,5,19,6],[19,7,19,8],[20,5,20,6],[20,7,20,8],[21,5,21,6],[21,7,21,8],[22,5,22,6],[22,7,22,8],[23,0,23,8],[25,6,25,8],[26,0,26,8],[27,0,27,7],[28,5,28,6],[28,7,28,8],[29,5,29,6],[29,7,29,8],[30,5,30,6],[30,7,30,8],[31,5,31,6],[31,7,31,8],[32,5,32,6],[32,7,32,8],[33,5,33,6],[33,7,33,8],[34,5,34,6],[34,7,34,8],[35,5,35,6],[35,7,35,8],[36,5,36,6],[36,7,36,8],[37,5,37,6],[37,7,37,8],[38,5,38,6],[38,7,38,8],[39,5,39,6],[39,7,39,8],[40,5,40,6],[40,7,40,8],[41,5,41,6],[41,7,41,8],[42,5,42,6],[42,7,42,8],[43,5,43,6],[43,7,43,8],[44,5,44,6],[44,7,44,8],[45,5,45,6],[45,7,45,8],[46,5,46,6],[46,7,46,8],[47,5,47,6],[47,7,47,8],[48,5,48,6],[48,7,48,8],[49,5,49,6],[49,7,49,8],[50,5,50,6],[50,7,50,8],[51,5,51,6],[51,7,51,8],[52,5,52,6],[52,7,52,8],[53,5,53,6],[53,7,53,8],[54,5,54,6],[54,7,54,8],[55,5,55,6],[55,7,55,8],[56,5,56,6],[56,7,56,8],[57,5,57,6],[57,7,57,8],[58,0,58,8]],"flags":["formulas_cached_only"]}
["安全文明措施费分解表"]
["工程名称：丰县大沙河水生态子午河水系贯通工程",{"$nulls":7},"第1页 共2页"]
["序号","项目名称","计量单位","数量","单价（元）","合价（元）",null,"备注"]
["一","完善、改造和维护安全防护设施设备","元",""]
["1","现场临时用电防护","元","",{"$nulls":3},"用电保护；高压区和用电危险区防护和围挡"]
["2","洞口、临边防护","元","",{"$nulls":3},"洞口、临边等危险部位防坠、防滑设施；临时防护盖板或围栏和隔离防护层"]
["3","机械设备防护","元","",{"$nulls":3},"钢防护网罩、防护挡板、防护栏杆等安全防护"]
["4","高处作业防护","元","",{"$nulls":3},"防止物体、人员坠落而设置的安全网、防护棚、防护栏杆、警戒线"]
["5","交叉作业防护","元","",{"$nulls":3},"平面、立面交叉作业时的防护"]
["6","防火、防爆、防尘、防毒","元",""]
["7","防雷、防台风、防地质灾害","元",""]
["8","地下工程有害气体监测、通风","元",""]
["9","临时安全防护","元","",{"$nulls":3},"围堰安全监测、防护，高脚手、高立模安全防护"]
["10","安全警示标志","元","",{"$nulls":3},"警告、提醒、指令、指示等标志、标牌；示警灯、报警闪光灯、夜间警示灯、照明灯"]
["二","配备、维护、保养应急救援器材、设备和应急演练","元",""]
["1","配备、维护、保养应急救援器材、设备","元","",{"$nulls":3},"应急救援器材、设备的配备、维护、保养和更新"]
["2","应急演练","元",""]
["三","重大危险源和事故隐患评估、监控和整改","元",""]
["1","重大危险源评估、监控与管理","元",""]
["2","事故隐患排查、评估和整改","元",""]
["四","安全文明生产检查、评价、咨询和标准化建设","元","",{"$nulls":3},"安全文明生产检查、评价、咨询和标准化建设持续改进等。不含企业安全生产标准化等级创建过程中给予咨询评价机构的评价咨询费用"]
["五","配备和更新现场作业人员安全防护用品","元","",{"$nulls":3},"必须配备的安全防护用品及对安全防护用品的正常损耗进行必要补充"]
["六","安全文明生产宣传、教育、培训","元","",{"$nulls":3},"安全文明宣传活动、标语、展板、音像、图片资料等；安全技术交底、安全操作规程培训、安全知识教育；知识竞赛、技能竞赛、专题会议；经验交流、现场观摩"]
[]
[]
[]
["安全文明措施费分解表"]
["工程名称：丰县大沙河水生态子午河水系贯通工程",{"$nulls":7},"第2页 共2页"]
["序号","项目名称","计量单位","数量","单价（元）","合价（元）",null,"备注"]
["七","安全文明生产适用的新技术、新标准、新工艺、新装备的推广应用","元",""]
["八","安全设施及特种设备检测检验","元",""]
["九","文明施工、生活设施和环境的改善、运行和维护","元",""]
["1","现场布置","元","",{"$nulls":3},"现场围挡、五板一图、企业标志"]
["2","办公和生活设施","元","",{"$nulls":3},"施工现场办公、生活区与作业区分开设置，保持安全距离；设施符合卫生和安全要求；文体卫生设施配备"]
["3","现场管理","元","",{"$nulls":3},"场容场貌；工地地面硬化处理等；材料堆放；扬尘控制；垃圾清运；环境美化、绿化；现场保洁"]
["十","其他与安全文明施工直接相关的内容","元","",{"$nulls":3},"含廉政建设费用"]
[null,"总计",null,""]